HT MICRON SEMICONDUTORES S.A.



Av. Unisinos, 1550 | 93022-750 | São Leopoldo | RS | Brasil

www.htmicron.com.br

|  |
| --- |
| AT-Commands Specification |
| Firmware Specification Document |
| Code: [Palavras-chave] |
| Doc. Type: Specification Document |
| Date: 02/12/2021 |
| Revision: PRELIMINARY |
| Classification: [Comentários] |

|  |
| --- |
| This document in a property of HT Micron and cannot be reproduced without its consent.  HT Micron does not assume any responsibility for use what is described.  This document is subject to change without notice.  No patent licenses are implied. |

SUMMARY

[TABLE SUMMARY 1](#_Toc93306458)

[DOCUMENT INFO 2](#_Toc93306459)

[REVISION 2](#_Toc93306460)

[APPROVAL 2](#_Toc93306461)

[2. AT command syntax 3](#_Toc93306462)

[3. General COmmands 3](#_Toc93306463)

[4. Default parameter state 3](#_Toc93306464)

[5. Device configuration 3](#_Toc93306465)

[**5.1. Key Configuration** 3](#_Toc93306466)

[**5.1.1. General Command** 3](#_Toc93306467)

[**5.1.2. ABP Keys Commands** 3](#_Toc93306468)

[**5.1.3. OTAA Keys Commands** 3](#_Toc93306469)

[**5.2. Region** 4](#_Toc93306470)

[**5.3. Activation Mode** 4](#_Toc93306471)

[**5.4. ADR** 4](#_Toc93306472)

[**5.5. Default TX Datarate** 4](#_Toc93306473)

[**5.6. Join Delay** 5](#_Toc93306474)

[**5.7. RX Window Delay** 5](#_Toc93306475)

[**5.8. RX Window Duration** 5](#_Toc93306476)

[**5.9. TX Power** 5](#_Toc93306477)

[**5.10. Add Channels** 6](#_Toc93306478)

[**5.11. Remove Channels** 7](#_Toc93306479)

[**5.12. Network Mode** 8](#_Toc93306480)

[6. Packet send/receive 8](#_Toc93306481)

[**6.1. Join Procedure** 8](#_Toc93306482)

[**6.2. Send Payload** 8](#_Toc93306483)

[**6.3. Receive Payload** 8](#_Toc93306484)

[7. Max Payload 8](#_Toc93306485)

[8. Default parameter state 8](#_Toc93306486)

[9. ERROR codes 9](#_Toc93306487)

[9.1. Command Error codes 9](#_Toc93306488)

[9.2. UART Error codes 9](#_Toc93306489)

[9.1. LORA Error codes 10](#_Toc93306490)

Table LIST

[Table 1 – Datarate Configurations 5](#_Toc93306287)

[Table 2 – Channel Configuration 7](#_Toc93306288)

[Table 3 – Maximum payload 8](#_Toc93306289)

[Table 4 – Default parameters 9](#_Toc93306290)

[Table 5 – Command error codes 9](#_Toc93306291)

[Table 6 – UART error codes 10](#_Toc93306292)

[Table 7 – LoRa error codes 10](#_Toc93306293)

# DOCUMENT INFO

This document provides information about the specifications of all blocks that will compose the system in package.

# REVISION

|  |  |  |  |
| --- | --- | --- | --- |
| Version | History | Date | Authors |
| 00 | - Initial draft | 02/12/2021 | Christian R Lehmen |
| 01 | Bug fixes and new features | 11/03/2022 | Christian R Lehmen |

# APPROVAL

|  |  |  |  |
| --- | --- | --- | --- |
| Position | Name | Date | Remarks |
|  |  |  |  |
|  |  |  |  |

# 

# Introduction

This application has the objective of making the first contact with the HTLRBL32L’s LoRaWAN® capabilities quick and easy using AT commands through a UART interface. The LoRaWAN version used on this application is [LoRaWAN 1.0.2rb](https://lora-alliance.org/resource_hub/lorawan-regional-parameters-v1-0-2rb/) and has all the features required to run on any LoRaWAN® network.

## **Serial Terminal Setup**

The UART interface can be used by connecting the pins TX(PA9) and RX(PA8) to a USB-Serial converter and connecting to a computer or simply connecting it to another microcontroller with a UART interface.

UART configuration required to connect:

* Baud rate: 115200
* Data bits: 8
* Stop bits: 1
* Parity: none
* Flow Control: none
* Transmitted text: Append LF

## **Termite Setup**

**One of the most widely used software for UART communication using a computer is** [Termite](https://www.compuphase.com/software_termite.htm)**.** Figure 1 – Termite setup **displays the configuration required to connect to the HTLRBL32L.**

Graphical user interface

Description automatically generated

Figure – Termite setup

# AT command syntax

|  |  |
| --- | --- |
| **Command** | **Description** |
| AT+CMD? | Read the parameter value |
| AT+CMD | Executes a command |
| AT+CMD=<parameters> | Executes a command with parameters |

# General COmmands

Returns the value input by the user. Command useful for UART connectivity tests.

|  |  |  |
| --- | --- | --- |
| **Command** | **Parameter** | **Description** |
| AT+ECHO=<param> | Any string value | Returns the input parameter |

# Device configuration

This section has all the commands necessary to configure the device.

## **Key Configuration**

Commands related to LoRaWAN ABP/OTAA key configuration.

### **General Command**

|  |  |  |
| --- | --- | --- |
| **Command** | **Parameter** | **Description** |
| AT+DEVEUI=<param> | 16 character hexadecimal | Sets the DevEUI |
| AT+DEVEUI? |  | Returns current DevEUI |

### **ABP Keys Commands**

ABP keys configuration is not required when using OTAA activation mode.

|  |  |  |
| --- | --- | --- |
| **Command** | **Parameter** | **Description** |
| AT+DEVADDR=<param> | 8 character hexadecimal | Sets the DevAddr |
| AT+DEVADDR? |  | Returns current DevAddr |
| AT+APPSKEY=<param> | 32 character hexadecimal | Sets the AppSKey |
| AT+APPSKEY? |  | Returns current AppSKey |
| AT+NWKSKEY=<param> | 32 character hexadecimal | Sets the NwkSKey |
| AT+NWKSKEY? |  | Returns current NwkSKey |

### **OTAA Keys Commands**

OTAAkeys configuration is not required when using ABP activation mode.

|  |  |  |
| --- | --- | --- |
| **Command** | **Parameter** | **Description** |
| AT+APPEUI=<param> | 16 character hexadecimal | Sets the AppEUI |
| AT+APPEUI? |  | Returns current AppEUI |
| AT+APPKEY=<param> | 32 character hexadecimal | Sets the AppKey |
| AT+APPKEY? |  | Returns current AppKey |

## **Region**

Sets the region of operation of the device. Regions set as RED are disabled in this version.

|  |  |  |
| --- | --- | --- |
| **Command** | **Parameter** | **Description** |
| AT+REGION=<param> | AS923 = 0  AU915 = 1  CN470 = 2  CN779 = 3  EU433 = 4  EU868 = 5  KR920 = 6  IN865 = 7  US915 = 8  RU864 = 9 | Sets the LoRaWAN Region |
| AT+ REGION? |  | Returns current Region |

## **Activation Mode**

Sets the join type (ABP/OTAA)

|  |  |  |
| --- | --- | --- |
| **Command** | **Parameter** | **Description** |
| AT+JOINCFG=<param> | ABP = 0, OTAA = 1 | Sets the join procedure type |
| AT+JOINCFG? |  | Returns the current join procedure type |

## **ADR**

Sets the ADR bit.

Note: Default Tx Datarate is ignored when the ADR bit is active

|  |  |  |
| --- | --- | --- |
| **Command** | **Parameter** | **Description** |
| AT+ADR=<param> | Off = 0, On = 1 | Sets the ADR bit |
| AT+ADR? |  | Returns current ADR config |

## **Default TX Datarate**

Default datarate is not used when ADR is activated.

|  |  |  |
| --- | --- | --- |
| **Command** | **Parameter** | **Description** |
| AT+DR=<param> | 0-7 | Sets the default datarate |
| AT+DR? |  | Returns default datarate |

Table 1 – Datarate Configurations displays the relation of Datarate with Spreading Factor and Bandwidth.

|  |  |  |  |
| --- | --- | --- | --- |
| **DR** | **AU915** | **US915** | **EU868** |
| 0 | SF12BW125 | SF10BW125 | SF12BW125 |
| 1 | SF11BW125 | SF9BW125 | SF11BW125 |
| 2 | SF10BW125 | SF8BW125 | SF10BW125 |
| 3 | SF9BW125 | SF7BW125 | SF9BW125 |
| 4 | SF8BW125 | SF8BW500 | SF8BW125 |
| 5 | SF7BW125 | Invalid | SF7BW125 |
| 6 | SF8BW500 | Invalid | SF7BW250 |
| 7 | Invalid | Invalid | FSK |

Table – Datarate Configurations

## **Join Delay**

Delay between Tx and opening the Rx1 and Rx2 windows during activation (used by OTAA activation mode)

|  |  |  |
| --- | --- | --- |
| **Command** | **Parameter** | **Description** |
| AT+JOINDELAYRX1=<param> | Time in milliseconds | Sets the join delay on the RX1 |
| AT+JOINDELAYRX1? |  | Returns the join delay on the RX1 |
| AT+JOINDELAYRX2=<param> | Time in milliseconds | Sets the join delay on the RX2 |
| AT+JOINDELAYRX2? |  | Returns the join delay on the RX2 |

## **RX Window Delay**

Delay between Tx and opening the Rx1 and Rx2 windows during regular execution.

|  |  |  |
| --- | --- | --- |
| **Command** | **Parameter** | **Description** |
| AT+DELAYRX1=<param> | Time in milliseconds | Sets the delay on the RX1 |
| AT+DELAYRX1? |  | Returns the delay on the RX1 |
| AT+DELAYRX2=<param> | Time in milliseconds | Sets the delay on the RX2 |
| AT+DELAYRX2? |  | Returns the delay on the RX2 |

## **RX Window Duration**

Sets the duration in which the Rx windows stay open (regular and join procedure RX windows). This rule must be respected when setting Rx window delays: **(Rx2Delay-Rx1Delay) >= (RxDuration** **+100).**

|  |  |  |
| --- | --- | --- |
| **Command** | **Parameter** | **Description** |
| AT+RXDURATION=<param> | Time in milliseconds | Sets the duration RX stays open |
| AT+RXDURATION? |  | Returns the set duration |

## **TX Power**

|  |  |  |
| --- | --- | --- |
| **Command** | **Parameter** | **Description** |
| AT+POWER=<param> | 0-15 | Sets the TX power level |
| AT+POWER? |  | Returns current TX power |

Tx power can be limited by regional specification, please refer to RP002-1.0.2 LoRaWAN Regional Parameters Document for more information.

## **Add Channels**

Command compatible with US915 and AU915 regions only.

|  |  |  |
| --- | --- | --- |
| **Command** | **Parameter** | **Description** |
| AT+CHMASK=<param> | param1:param2:param3...\* | Adds channels to the channel mask |
| AT+CHMASK? |  | Returns current channel mask |

\*Maximum of 8 channels per command (e.g: AT+CHMASK=1:2:3:4:5:10:25:8)

The frequency each channel represents in the device is depicted on Table 2 – Channel Configuration.

|  |  |  |
| --- | --- | --- |
| **Channel n°** | **AU915** | **US915** |
| 1 | 915200000 | 902300000 |
| 2 | 915400000 | 902500000 |
| 3 | 915600000 | 902700000 |
| 4 | 915800000 | 902900000 |
| 5 | 916000000 | 903100000 |
| 6 | 916200000 | 903300000 |
| 7 | 916400000 | 903500000 |
| 8 | 916600000 | 903700000 |
| 9 | 916800000 | 903900000 |
| 10 | 917000000 | 904100000 |
| 11 | 917200000 | 904300000 |
| 12 | 917400000 | 904500000 |
| 13 | 917600000 | 904700000 |
| 14 | 917800000 | 904900000 |
| 15 | 918000000 | 905100000 |
| 16 | 918200000 | 905300000 |
| 17 | 918400000 | 905500000 |
| 18 | 918600000 | 905700000 |
| 19 | 918800000 | 905900000 |
| 20 | 919000000 | 906100000 |
| 21 | 919200000 | 906300000 |
| 22 | 919400000 | 906500000 |
| 23 | 919600000 | 906700000 |
| 24 | 919800000 | 906900000 |
| 25 | 920000000 | 907100000 |
| 26 | 920200000 | 907300000 |
| 27 | 920400000 | 907500000 |
| 28 | 920600000 | 907700000 |
| 29 | 920800000 | 907900000 |
| 30 | 921000000 | 908100000 |
| 31 | 921200000 | 908300000 |
| 32 | 921400000 | 908500000 |
| 33 | 921600000 | 908700000 |
| 34 | 921800000 | 908900000 |
| 35 | 922000000 | 909100000 |
| 36 | 922200000 | 909300000 |
| 37 | 922400000 | 909500000 |
| 38 | 922600000 | 909700000 |
| 39 | 922800000 | 909900000 |
| 40 | 923000000 | 910100000 |
| 41 | 923200000 | 910300000 |
| 42 | 923400000 | 910500000 |
| 43 | 923600000 | 910700000 |
| 44 | 923800000 | 910900000 |
| 45 | 924000000 | 911100000 |
| 46 | 924200000 | 911300000 |
| 47 | 924400000 | 911500000 |
| 48 | 924600000 | 911700000 |
| 49 | 924800000 | 911900000 |
| 50 | 925000000 | 912100000 |
| 51 | 925200000 | 912300000 |
| 52 | 925400000 | 912500000 |
| 53 | 925600000 | 912700000 |
| 54 | 925800000 | 912900000 |
| 55 | 926000000 | 913100000 |
| 56 | 926200000 | 913300000 |
| 57 | 926400000 | 913500000 |
| 58 | 926600000 | 913700000 |
| 59 | 926800000 | 913900000 |
| 60 | 927000000 | 914100000 |
| 61 | 927200000 | 914300000 |
| 62 | 927400000 | 914500000 |
| 63 | 927600000 | 914700000 |
| 64 | 927800000 | 914900000 |
| 65 | 915900000 | 903000000 |
| 66 | 917500000 | 904600000 |
| 67 | 919100000 | 906200000 |
| 68 | 920700000 | 907800000 |
| 69 | 922300000 | 909400000 |
| 70 | 923900000 | 911000000 |
| 71 | 925500000 | 912600000 |
| 72 | 927100000 | 914200000 |

Table – Channel Configuration

Channels 65-72 are used by exclusively on DR6(AU915) and DR4(US915).

## **Remove Channels**

Command compatible with US915 and AU915 regions only.

|  |  |  |
| --- | --- | --- |
| **Command** | **Parameter** | **Description** |
| AT+RMVCHMASK=<param> | param1:param2:param3...\* | Removes channels from the channel mask |
| AT+CHMASK? |  | Returns current channel mask |

\*Maximum of 8 channels per command (e.g: AT+RMVCHMASK=1:2:3:4:5:10:25:8)

\*Sending a “AT+RMVCHMASK=0” command will revert the channel mask to its default state.

## **Network Mode**

|  |  |  |
| --- | --- | --- |
| **Command** | **Parameter** | **Description** |
| AT+NWKMODE=<param> | 0: private mode  1: public mode | Sets network mode |
| AT+NWKMODE? |  | Returns current network mode |

# Packet send/receive

## **Join Procedure**

Performs the join procedure, exchanging keys required to communicate with the network server. Command is **required** to be used once before sending a payload if Network Join Type is OTAA.

|  |  |  |
| --- | --- | --- |
| **Command** | **Parameter** | **Description** |
| AT+NWKJOIN |  | Sends a join request |
| AT+NWKJOIN? |  | Return join status |

## 

## **Send Payload (String)**

Sends an uplink to the network server containing a user payload. Automatically opens both RX windows to expect a downlink.

|  |  |  |
| --- | --- | --- |
| **Command** | **Parameter** | **Description** |
| AT+SEND=<param> | 1-242 bytes payload\* | Sends a packet |

\*Payload size is dependent on current Datarate, refer to item 7 (Max Payload) for the appropriate values.

## **Send Payload (Hexadecimal)**

Sends an uplink to the network server containing a hexadecimal user payload. Automatically opens both RX windows to expect a downlink.

|  |  |  |
| --- | --- | --- |
| **Command** | **Parameter** | **Description** |
| AT+SENDHEX=<param> | 1-242 bytes payload\* | Sends a packet |

\*Payload size is dependent on current Datarate, refer to item 7 (Max Payload) for the appropriate values.

## **Receive Payload**

Returns the last application payload received by downlink. If there is no payload received or it has already been read an error is reported. Only payload addressed to LoRaWAN port 2 are returned.

|  |  |  |
| --- | --- | --- |
| **Command** | **Parameter** | **Description** |
| AT+RCV |  | Returns the last received payload |

## 

## **Rx Stats**

Returns the last received packet stats (RSSI/SNR) on this format: <RSSI> <SNR>.

|  |  |  |
| --- | --- | --- |
| **Command** | **Parameter** | **Description** |
| AT+STATS? |  | Returns RSSI and SNR of the last packet received |

# Max Payload

Table 3 – Maximum payload displays the maximum payload allowed for each datarate of each region (value in bytes).

|  |  |  |  |
| --- | --- | --- | --- |
| **Datarate** | **AU915** | **EU868** | **US915** |
| 0 | 51 | 51 | 11 |
| 1 | 51 | 51 | 53 |
| 2 | 51 | 51 | 125 |
| 3 | 115 | 115 | 242 |
| 4 | 242 | 242 | 242 |
| 5 | 242 | 242 | Invalid |
| 6 | 242 | 242 | Invalid |
| 7 | Invalid | 242 | Invalid |

Table – Maximum payload

# Default parameter state

When the system is initialized/reset all parameters go to their default state, depicted on the Table 4 – Default parameters.

|  |  |
| --- | --- |
| **Parameter** | **Value** |
| DevEUI | 0xDEADBEEFBEEFDEAD |
| DevAddr | 0xDEADBEEF |
| AppSkey | 0x11111111111111111111111111111111 |
| NwkSkey | 0x11111111111111111111111111111111 |
| AppEUI | 0x1111111111111111 |
| AppKey | 0x11111111111111111111111111111111 |
| Active Channels | 9-16 |
| Join Configuration | ABP |
| ADR | 0 |
| Network Mode | 1 |
| Default Datarate | 0 |
| Join Delay Rx1 | 5000 |
| Join Delay Rx2 | 6000 |
| Delay Rx1 | 1000 |
| Delay Rx2 | 2000 |
| Rx Window Size | 850 |
| Tx Power | 14 |
| Region | US915 |

Table – Default parameters

# ERROR codes

After every command and during special events the system will return a hexadecimal 4-byte error code referring to possible errors during the execution, using this format:

[00][00][00][00]

Reserved

CMD

LORA

UART

## **Command Error codes**

The first byte is related to command syntax and parameter validations.

|  |  |
| --- | --- |
| **Code** | **Description** |
| 0x00 | No errors |
| 0x01 | Invalid command |
| 0x02 | Parameter missing |
| 0x03 | Parameter overflow |
| 0x04 | Invalid command header |
| 0x05 | Expected hexadecimal value |

Table – Command error codes

## **UART Error codes**

The second byte is related to possible UART errors.

|  |  |
| --- | --- |
| **Code** | **Description** |
| 0x00 | No errors |
| 0x01 | Command max size violated |
| 0x02 | Empty command |

Table – UART error codes

## **LORA Error codes**

The third byte refers to LoRa errors.

|  |  |
| --- | --- |
| **Code** | **Description** |
| 0x00 | No errors |
| 0x01 | Invalid region |
| 0x02 | Invalid Rx Window configuration¹ |
| 0x03 | Network already joined |
| 0x04 | Invalid payload size |
| 0x05 | Invalid payload+FOPTS size² |
| 0x06 | No new Rx Data |
| 0x07 | LoRaWAN stack error³ |
| 0x08 | Tx Timeout |

Table – LoRa error codes

¹ - (Rx2 Window Delay - Rx1 Window Delay) must be greater than (Rx Window size + 100).

Eg:   
Rx2Delay = 1000.

Rx1Delay = 2000.

RxDuration = 850.

(Rx2Delay-Rx1Delay) >= (RxDuration +100) **OK**

Eg:   
Rx2Delay = 1000.

Rx1Delay = 2000.

RxDuration = 1500.

(Rx2Delay-Rx1Delay) >= (RxDuration +100) **ERROR**

² - Application Payload plus LoRaWAN configuration commands exceeds max payload size. This error can be reported dynamically during execution. When this error happens, the packet is sent without the application payload.

³ - Internal LoRaWAN stack error. After this error the stack is reset (user configuration is maintained)